Pöttinger presents new grassland products

Grassland specialist Pöttinger has once again tied up a colourful bouquet of innovations for the new season. There is something new for every link in the harvesting chain: from mowing, tedding and raking to loading.

NOVACAT V 10000: The new standard in mowing

The new mower combination combines high output with the best possible ground tracking and the greatest reliability thanks to intelligent technology. The NOVACAT V 10000 is available with a headstock for 3.0 or 3.5 metre wide front mowers. This makes working widths of up to 9.62 and 10.02 metres possible.

|  |  |
| --- | --- |
| Ein Bild, das Gras, draußen, Himmel, Feld enthält.  Automatisch generierte Beschreibung | Ein Bild, das Gras, draußen, Himmel, Feld enthält.  Automatisch generierte Beschreibung |
| The mower combination  NOVACAT V 10000 defines a new standard in mowing | NOVACAT V 10000  Mower combination for the best  working results |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5195> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5194> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/NOVACAT_V_10000_EN_2022-06.docx>

New HIT V 11100 – Powerful and compact

With its 1.42 metre rotors and 10.70 metre working width (DIN), the HIT V 11100 combines excellent tedding quality with maximum output. While the HIT is inconspicuously small during transport, it unfolds to reveal stunning dimensions in the field. It also boasts an impressive array of technical refinements.

|  |  |
| --- | --- |
|  |  |
| The new HIT V 11100 is in a class of its own | The compact HIT V 11100 delivers the best working results |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5202> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5201> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/HIT_V_11100_EN_2022-06.docx>

TOP 882 C: The new large centre-swath rake

Pöttinger has added the new TOP 882 C to their range of popular centre-swath rakes. The TOP 882 C demonstrates its full capabilities at a working width of 7.70 to 8.80 metres. The longer boom allows very flexible swath width adjustment between 1.30 and 2.60 metres. Flexibility that offers the advantage of wider swaths for forage harvesters and narrower swath widths for small loader wagons. Despite the impressive rotor diameter of 3.70 metres, the transport height without removing the tine arms is still below 4.00 metres.

|  |  |
| --- | --- |
| Ein Bild, das Gras, draußen, Feld, Himmel enthält.  Automatisch generierte Beschreibung | Ein Bild, das Text, Gras, Pflanze enthält.  Automatisch generierte Beschreibung |
| The new TOP 882 C centre-swath rake demonstrates its full capabilities with job-specific working widths | TOP 882 C: The new large centre-swath rake |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5196> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5197> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/TOP_882_C_EN_2022-06.docx>

New belt-type rake MERGENTO VT 9220

The new MERGENTO VT 9220 belt-type rake (with working widths of up to 9.20 metres for a central swath and 8.70 metres for a side swath) is designed for alfalfa, clover, and a wide variety of crops from permanent grassland to straw. MERGENTO collects the forage using the pick-up. Without further contact with the ground, cross conveyor belts transport the forage to the swath.

|  |  |
| --- | --- |
| Ein Bild, das Gras, draußen, Landmaschine enthält.  Automatisch generierte Beschreibung | Ein Bild, das Gras, draußen, Feld, grasbedeckt enthält.  Automatisch generierte Beschreibung |
| The new MERGENTO VT 9220 belt rake is the specialist for all types of forage | The new MERGENTO with innovative features |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5193> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5192> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/MERGENTO_VT_9220_EN_2022-06.docx>

The new JUMBO 8000 chops much shorter

With the new short chop system, the world market leader in loader wagons has taken another step further. The new JUMBO 8000 chops the forage almost 30 percent shorter: This means even higher forage quality without compromising on loading performance. Protected to a torque of 3,500 Nm, the loader wagon can now deliver higher throughput rates than a self-propelled forage harvester.

|  |  |
| --- | --- |
| Ein Bild, das Gras, draußen, Himmel, LKW enthält.  Automatisch generierte Beschreibung | Ein Bild, das Pflanze, grün, Konifere enthält.  Automatisch generierte Beschreibung |
| The new JUMBO 8450 with short-chop chopping system | Perfect chopped length |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5073> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5075> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/JUMBO_Short_chop_EN_2022-03.docx>

Contactless steered axles on the JUMBO

Agricultural machinery manufacturer Pöttinger underlines its world market leadership in loader wagons with innovative developments to its flagship, the JUMBO: Convenience and safety have a very high priority. The new contactless, electronic steered axles on the JUMBO loader wagon significantly improve operating and driving comfort as well as the reliability of the steering system.

Developed together with ME MOBIL ELEKTRONIK GMBH, the system was launched on the JUMBO loader wagon first.

|  |  |
| --- | --- |
| Ein Bild, das Gras, draußen, Himmel, Outdoorobjekt enthält.  Automatisch generierte Beschreibung | Ein Bild, das Himmel, draußen, Tag enthält.  Automatisch generierte Beschreibung |
| The contactless electronic steered axle system enables a tight turning angle | The new JUMBO with innovative features on board |
| <https://www.poettinger.at/de_at/Newsroom/Pressebild/5076> | <https://www.poettinger.at/de_at/Newsroom/Pressebild/5077> |

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/JUMBO_Contactless_EN_2022-06.docx>

BOSS 3000 MASTER, the new benchmark

The BOSS 3000 MASTER complements the product range of loader wagons for smaller scale farm businesses and farms in the foothills of the Alps. The engineers have succeeded in reducing maintenance requirements to a minimum with a loading unit developed from the ground up, while at the same time significantly increasing throughput capacity. In addition, new smart options, previously only available on the larger wagons, are now also available for the BOSS. It is available in four sizes from 18.7 to 26.5 m³ (DIN). Two of them also with beater rotors. The BOSS 3000 MASTER series is available from 01 August 2022.

Ein Bild, das Gras, draußen, Himmel, Outdoorobjekt enthält.

Automatisch generierte Beschreibung

BOSS 3000 MASTER, the new benchmark for small farms

<https://www.poettinger.at/de_at/Newsroom/Pressebild/5191>

**To the long version:**

<https://www.poettinger.at/landtechnik/download/pressetexte/BOSS_3000_MASTER_EN_2022-06.docx>